#!/bin/bash

[ -z "$CRYPTSETUP_PATH" ] && CRYPTSETUP_PATH=".."
CRYPTSETUP=$CRYPTSETUP_PATH/cryptsetup
DEV=""
DEV_STACKED="luks0xbabe"
DEV_NAME="dummyalign"
HDR="test_luks2_hdr"
MNT_DIR="./mnt_luks"
PWD1="93R4P4pIqAH8"
PWD2="mymJeD8ivEhE"
FAST_PBKDF="--pbkdf pbkdf2 --pbkdf-force-iterations 1000"

if [ -n "$CRYPTSETUP_TESTS_RUN_IN_MESON" ]; then
	CRYPTSETUP_VALGRIND=$CRYPTSETUP
else
	CRYPTSETUP_VALGRIND=../.libs/cryptsetup
	CRYPTSETUP_LIB_VALGRIND=../.libs
fi

cleanup() {
	udevadm settle >/dev/null 2>&1
	if [ -d "$MNT_DIR" ] ; then
		umount -f $MNT_DIR 2>/dev/null
		rmdir $MNT_DIR 2>/dev/null
	fi
	[ -b /dev/mapper/$DEV_STACKED ] && dmsetup remove --retry $DEV_STACKED >/dev/null 2>&1
	[ -b /dev/mapper/$DEV_NAME ] && dmsetup remove --retry $DEV_NAME >/dev/null 2>&1
	# FIXME scsi_debug sometimes in-use here
	sleep 1
	rmmod scsi_debug >/dev/null 2>&1
	sleep 1
	rm -f $HDR 2>/dev/null
}

fail()
{
	if [ -n "$1" ] ; then echo "FAIL $1" ; fi
	echo "FAILED backtrace:"
	while caller $frame; do ((frame++)); done
	cleanup
	exit 100
}

skip()
{
	echo "TEST SKIPPED: $1"
	cleanup
	exit 77
}

function valgrind_setup()
{
	command -v valgrind >/dev/null || fail "Cannot find valgrind."
	[ ! -f $CRYPTSETUP_VALGRIND ] && fail "Unable to get location of cryptsetup executable."
	[ ! -f valg.sh ] && fail "Unable to get location of valg runner script."
	if [ -z "$CRYPTSETUP_TESTS_RUN_IN_MESON" ]; then
		export LD_LIBRARY_PATH="$CRYPTSETUP_LIB_VALGRIND:$LD_LIBRARY_PATH"
	fi
}

function valgrind_run()
{
	INFOSTRING="$(basename ${BASH_SOURCE[1]})-line-${BASH_LINENO[0]}" ./valg.sh ${CRYPTSETUP_VALGRIND} "$@"
}

function dm_crypt_features()
{
	VER_STR=$(dmsetup targets | grep crypt | cut -f2 -dv)
	[ -z "$VER_STR" ] && fail "Failed to parse dm-crypt version."

	VER_MAJ=$(echo $VER_STR | cut -f 1 -d.)
	VER_MIN=$(echo $VER_STR | cut -f 2 -d.)
	VER_PTC=$(echo $VER_STR | cut -f 3 -d.)

	[ $VER_MAJ -lt 1 ] && return
	[ $VER_MAJ -gt 1 ] && {
		DM_PERF_CPU=1
		DM_SECTOR_SIZE=1
		return
	}

	[ $VER_MIN -lt 14 ] && return
	DM_PERF_CPU=1
	if [ $VER_MIN -ge 17 ]; then
		DM_SECTOR_SIZE=1
	fi
}

add_device() {
	modprobe scsi_debug $@ delay=0 >/dev/null 2>&1
	if [ $? -ne 0 ] ; then
		echo "This kernel seems to not support proper scsi_debug module, test skipped."
		exit 77
	fi

	sleep 1
	DEV=$(grep -l -e scsi_debug /sys/block/*/device/model | cut -f4 -d /)

	if [ ! -e /sys/block/$DEV/alignment_offset ] ; then
		echo "This kernel seems to not support topology info, test skipped."
		cleanup
		exit 77
	fi

	DEV="/dev/$DEV"
	[ -b $DEV ] || fail "Cannot find $DEV."
}

format() # expected [forced] [encryption_sector_size]
{
	local _sec_size=512

	local _exp=$1

	if [ "${2:0:1}" = "s" ]; then
		_sec_size=${2:1}
		shift
	fi

	test "${3:0:1}" = "s" && _sec_size=${3:1}

	test $_sec_size -eq 512 || local _smsg=" (encryption sector size $_sec_size)"

	if [ -z "$2" ] ; then
		echo -n "Formatting using topology info$_smsg..."
		echo $PWD1 | $CRYPTSETUP luksFormat $FAST_PBKDF --type luks2 $DEV -q -c aes-cbc-essiv:sha256 --sector-size $_sec_size >/dev/null 2>&1 || fail
	else
		echo -n "Formatting using forced sector alignment $2$_smsg..."
		echo $PWD1 | $CRYPTSETUP luksFormat $FAST_PBKDF --type luks2 $DEV -q -c aes-cbc-essiv:sha256 --align-payload=$2 --sector-size $_sec_size >/dev/null || fail
	fi

	# check the device can be activated
	if [ -n "$DM_SECTOR_SIZE" ] ; then
		echo $PWD1 | $CRYPTSETUP luksOpen $DEV $DEV_NAME || fail
		$CRYPTSETUP close $DEV_NAME || fail
	fi

	ALIGN=$($CRYPTSETUP luksDump $DEV | grep -A1 "0: crypt" | grep "offset:" | cut -d ' ' -f2)
	# echo "ALIGN = $ALIGN"

	[ -z "$ALIGN" ] && fail
	ALIGN=$((ALIGN/512))
	[ $ALIGN -ne $_exp ] && fail "Expected alignment differs: expected $_exp != detected $ALIGN"

	# test some operation, just in case
	echo -e "$PWD1\n$PWD2" | $CRYPTSETUP luksAddKey $DEV $FAST_PBKDF --new-key-slot 1
	[ $? -ne 0 ] && fail "Keyslot add failed."

	$CRYPTSETUP -q luksKillSlot $DEV 1
	[ $? -ne 0 ] && fail "Keyslot removal failed."

	echo "PASSED"
}

format_fail() # expected [forced] [encryption_sector_size]
{
	local _sec_size=512

	local _exp=$1

	if [ "${2:0:1}" = "s" ]; then
		_sec_size=${2:1}
		shift
	fi

	test "${3:0:1}" = "s" && _sec_size=${3:1}

	test $_sec_size -eq 512 || local _smsg=" (encryption sector size $_sec_size)"

	if [ -z "$2" ] ; then
		echo -n "Formatting using topology info$_smsg (must fail)..."
		echo $PWD1 | $CRYPTSETUP luksFormat $FAST_PBKDF --type luks2 $DEV -q -c aes-cbc-essiv:sha256 --sector-size $_sec_size >/dev/null 2>&1 && fail
	else
		echo -n "Formatting using forced sector alignment $2$_smsg (must fail)..."
		echo $PWD1 | $CRYPTSETUP luksFormat $FAST_PBKDF --type luks2 $DEV -q -c aes-cbc-essiv:sha256 --align-payload=$2 --sector-size $_sec_size >/dev/null 2>&1 && fail
	fi

	echo "PASSED"
}

auto_sector() # expected device header
{
	local _exp=$1
	local _dev=$2
	local _hdr=$2
	local _hdrstr=""
	local _hdrmsg=""

	if [ -n "$3" ]; then
		_hdrstr="--header $3"
		_hdr=$3
		_hdrmsg=" detached header"
	fi

	echo -n "Formatting$_hdrmsg using optimal encryption sector size (expecting $_exp)..."

	if [ -z "$DM_SECTOR_SIZE" -a $_exp -ne 512 ]; then
		echo "SKIPPED"
		return
	fi

	echo $PWD1 | $CRYPTSETUP luksFormat $FAST_PBKDF --type luks2 $_hdrstr $_dev -q >/dev/null 2>&1 || fail

	# check the device can be activated
	echo $PWD1 | $CRYPTSETUP luksOpen $_hdrstr $_dev $DEV_NAME || fail
	$CRYPTSETUP close $DEV_NAME || fail

	SECTOR=$($CRYPTSETUP luksDump $_hdr | grep -A4 "0: crypt" | grep "sector:" | cut -d ' ' -f2)

	[ -z "$SECTOR" ] && fail
	[ $SECTOR -ne $_exp ] && fail "Expected sector size differs: expected $_exp != detected $SECTOR"

	echo "PASSED"
}

[ ! -x "$CRYPTSETUP" ] && skip "Cannot find $CRYPTSETUP, test skipped."
[ -n "$VALG" ] && valgrind_setup && CRYPTSETUP=valgrind_run
if [ $(id -u) != 0 ]; then
	echo "WARNING: You must be root to run this test, test skipped."
	exit 77
fi

dm_crypt_features
modprobe --dry-run scsi_debug >/dev/null 2>&1 || skip "This kernel seems to not support proper scsi_debug module, test skipped."
cleanup
if [ -d /sys/module/scsi_debug ] ; then
	echo "Cannot use scsi_debug module (in use or compiled-in), test skipped."
	exit 77
fi

add_device dev_size_mb=32
echo $PWD1 | $CRYPTSETUP luksFormat $FAST_PBKDF --type luks2 $DEV -q  >/dev/null || fail
EXPCT=$($CRYPTSETUP luksDump $DEV | grep "offset: " | cut -f 2 -d ' ')
test "$EXPCT" -gt 512 || fail
EXPCT=$((EXPCT/512))
echo "Default alignment detected: $EXPCT sectors"
cleanup

echo "# Create desktop-class 4K drive"
echo "# (logical_block_size=512, physical_block_size=4096, alignment_offset=0)"
add_device dev_size_mb=32 sector_size=512 physblk_exp=3 num_tgts=1
format $EXPCT
format $EXPCT s1024
format $EXPCT s2048
format $EXPCT s4096
format $EXPCT 1
format $EXPCT 1 s1024
format $EXPCT 1 s2048
format $EXPCT 1 s4096
format $EXPCT 8
format $EXPCT 8 s1024
format $EXPCT 8 s2048
format $EXPCT 8 s4096
format $((EXPCT+1)) $((EXPCT+1))
format_fail $((EXPCT+1)) $((EXPCT+1)) s1024
format_fail $((EXPCT+1)) $((EXPCT+1)) s2048
format_fail $((EXPCT+1)) $((EXPCT+1)) s4096
format $EXPCT $EXPCT
format $EXPCT $EXPCT s1024
format $EXPCT $EXPCT s2048
format $EXPCT $EXPCT s4096
cleanup

echo "# Create desktop-class 4K drive with misaligned opt-io (some bad USB enclosures)"
echo "# (logical_block_size=512, physical_block_size=4096, alignment_offset=0, opt-io=1025)"
add_device dev_size_mb=32 sector_size=512 physblk_exp=3 num_tgts=1 opt_blks=1025
format $EXPCT
format $EXPCT s1024
format $EXPCT s2048
format $EXPCT s4096
format $EXPCT 1
format $EXPCT 1 s1024
format $EXPCT 1 s2048
format $EXPCT 1 s4096
format $EXPCT 8
format $EXPCT 8 s1024
format $EXPCT 8 s2048
format $EXPCT 8 s4096
format $((EXPCT+1)) $((EXPCT+1))
format_fail $((EXPCT+1)) $((EXPCT+1)) s1024
format_fail $((EXPCT+1)) $((EXPCT+1)) s2048
format_fail $((EXPCT+1)) $((EXPCT+1)) s4096
format $EXPCT $EXPCT
format $EXPCT $EXPCT s1024
format $EXPCT $EXPCT s2048
format $EXPCT $EXPCT s4096
cleanup

echo "# Create drive with misaligned opt-io to page-size (some bad USB enclosures)"
echo "# (logical_block_size=512, physical_block_size=512, alignment_offset=0, opt-io=33553920)"
add_device dev_size_mb=32 sector_size=512 num_tgts=1 opt_blks=65535
format $EXPCT
format $EXPCT s1024
format $EXPCT s2048
format $EXPCT s4096
format $EXPCT 1
format $EXPCT 1 s1024
format $EXPCT 1 s2048
format $EXPCT 1 s4096
format $EXPCT 8
format $EXPCT 8 s1024
format $EXPCT 8 s2048
format $EXPCT 8 s4096
format $((EXPCT+1)) $((EXPCT+1))
format_fail $((EXPCT+1)) $((EXPCT+1)) s1024
format_fail $((EXPCT+1)) $((EXPCT+1)) s2048
format_fail $((EXPCT+1)) $((EXPCT+1)) s4096
format $EXPCT $EXPCT
format $EXPCT $EXPCT s1024
format $EXPCT $EXPCT s2048
format $EXPCT $EXPCT s4096
cleanup

echo "# Create desktop-class 4K drive w/ 1-sector shift (original bug report)"
echo "# (logical_block_size=512, physical_block_size=4096, alignment_offset=512)"
add_device dev_size_mb=32 sector_size=512 physblk_exp=3 lowest_aligned=1 num_tgts=1
format $((EXPCT+1))
format_fail $((EXPCT+1)) s1024
format_fail $((EXPCT+1)) s2048
format_fail $((EXPCT+1)) s4096
format $EXPCT 1
format $EXPCT 1 s1024
format $EXPCT 1 s2048
format $EXPCT 1 s4096
format $EXPCT 8
format $EXPCT 8 s1024
format $EXPCT 8 s2048
format $EXPCT 8 s4096
format $((EXPCT+1)) $((EXPCT+1))
format_fail $((EXPCT+1)) $((EXPCT+1)) s1024
format_fail $((EXPCT+1)) $((EXPCT+1)) s2048
format_fail $((EXPCT+1)) $((EXPCT+1)) s4096
format $EXPCT $EXPCT
format $EXPCT $EXPCT s1024
format $EXPCT $EXPCT s2048
format $EXPCT $EXPCT s4096
cleanup

echo "# Create desktop-class 4K drive w/ 63-sector DOS partition compensation"
echo "# (logical_block_size=512, physical_block_size=4096, alignment_offset=3584)"
add_device dev_size_mb=32 sector_size=512 physblk_exp=3 lowest_aligned=7 num_tgts=1
format $((EXPCT+7))
format_fail $((EXPCT+7)) s1024
format_fail $((EXPCT+7)) s2048
format_fail $((EXPCT+7)) s4096
format $EXPCT 1
format $EXPCT 1 s1024
format $EXPCT 1 s2048
format $EXPCT 1 s4096
format $EXPCT 8
format $EXPCT 8 s1024
format $EXPCT 8 s2048
format $EXPCT 8 s4096
format $((EXPCT+1)) $((EXPCT+1))
format_fail $((EXPCT+1)) $((EXPCT+1)) s1024
format_fail $((EXPCT+1)) $((EXPCT+1)) s2048
format_fail $((EXPCT+1)) $((EXPCT+1)) s4096
format $EXPCT $EXPCT
format $EXPCT $EXPCT s1024
format $EXPCT $EXPCT s2048
format $EXPCT $EXPCT s4096
cleanup

echo "# Create enterprise-class 4K drive"
echo "# (logical_block_size=4096, physical_block_size=4096, alignment_offset=0)"
add_device dev_size_mb=32 sector_size=4096 num_tgts=1 opt_blks=64
format $EXPCT
format $EXPCT s1024
format $EXPCT s2048
format $EXPCT s4096
format $EXPCT 1
format $EXPCT 1 s1024
format $EXPCT 1 s2048
format $EXPCT 1 s4096
format $EXPCT 8
format $EXPCT 8 s1024
format $EXPCT 8 s2048
format $EXPCT 8 s4096
#FIXME: kernel limits issue?
##format $((EXPCT+1)) $((EXPCT+1))
format_fail $((EXPCT+1)) $((EXPCT+1)) s1024
format_fail $((EXPCT+1)) $((EXPCT+1)) s2048
format_fail $((EXPCT+1)) $((EXPCT+1)) s4096
format $EXPCT $EXPCT
format $EXPCT $EXPCT s1024
format $EXPCT $EXPCT s2048
format $EXPCT $EXPCT s4096
cleanup

echo "# Create classic 512B drive and stack dm-linear"
echo "# (logical_block_size=512, physical_block_size=512, alignment_offset=0)"
add_device dev_size_mb=32 sector_size=512 num_tgts=1
DEV2=$DEV
DEV=/dev/mapper/$DEV_STACKED
dmsetup create $DEV_STACKED --table "0 65536 linear $DEV2 0"
format $EXPCT
format $EXPCT s1024
format $EXPCT s2048
format $EXPCT s4096
format $EXPCT 1
format $EXPCT 1 s1024
format $EXPCT 1 s2048
format $EXPCT 1 s4096
format $EXPCT 8
format $EXPCT 8 s1024
format $EXPCT 8 s2048
format $EXPCT 8 s4096
format $((EXPCT+1)) $((EXPCT+1))
format_fail $((EXPCT+1)) $((EXPCT+1)) s1024
format_fail $((EXPCT+1)) $((EXPCT+1)) s2048
format_fail $((EXPCT+1)) $((EXPCT+1)) s4096
format $EXPCT $EXPCT
format $EXPCT $EXPCT s1024
format $EXPCT $EXPCT s2048
format $EXPCT $EXPCT s4096
cleanup

echo "# Create enterprise-class 4K drive with fs and LUKS images."
# loop device here presents 512 block but images have 4k block
# cryptsetup should properly use 4k block on direct-io
add_device dev_size_mb=32 sector_size=4096 physblk_exp=0 num_tgts=1 opt_blks=64
for file in $(ls img_fs_*.img.xz) ; do
	echo -n "Format using fs image $file. "
	xz -d -c $file | dd of=$DEV bs=1M 2>/dev/null || fail "bad image"
	[ ! -d $MNT_DIR ] && mkdir $MNT_DIR
	mount $DEV $MNT_DIR 2>/dev/null
	if [ $? -ne 0 ] ; then
		echo "[N/A]"
		continue
	fi
	echo $PWD1 | $CRYPTSETUP luksFormat $FAST_PBKDF --type luks2 $MNT_DIR/luks.img --offset 8192 || fail
	echo $PWD2 | $CRYPTSETUP luksFormat $FAST_PBKDF --type luks2 $MNT_DIR/luks.img --header $MNT_DIR/luks_header.img || fail
	umount $MNT_DIR || fail
	echo "[OK]"
done
cleanup

echo "# Create classic 512B drive"
echo "# (logical_block_size=512, physical_block_size=512, alignment_offset=0)"
add_device dev_size_mb=32 sector_size=512 num_tgts=1
auto_sector 512 $DEV
auto_sector 512 $DEV $HDR
cleanup
echo "# Create desktop-class 4K drive"
echo "# (logical_block_size=512, physical_block_size=4096, alignment_offset=0)"
add_device dev_size_mb=32 sector_size=512 physblk_exp=3 num_tgts=1
auto_sector 4096 $DEV
auto_sector 4096 $DEV $HDR
DEV2=$DEV
DEV=/dev/mapper/$DEV_STACKED
dmsetup create $DEV_STACKED --table "0 $((`blockdev --getsz $DEV2`-1)) linear $DEV2 0"
auto_sector 512 $DEV
auto_sector 512 $DEV $HDR
cleanup
echo "# Create enterprise-class 4K drive"
echo "# (logical_block_size=4096, physical_block_size=4096, alignment_offset=0)"
add_device dev_size_mb=32 sector_size=4096 num_tgts=1 opt_blks=64
auto_sector 4096 $DEV
auto_sector 4096 $DEV $HDR
cleanup

exit 0
