(footprint "tht_vertical_potentiometer" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 61F777D4)
  (descr "Potentiometer, horizontally mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, http://www.alps.com/prod/info/E/HTML/Potentiometer/RotaryPotentiometers/RK09K/RK09D1130C1B.html")
  (tags "Potentiometer horizontal  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single")
  (attr through_hole)
  (fp_text reference "RV2" (at 2.5 0.5 -270) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1c222724-bc7c-4c84-b7e1-717621c5487e)
  )
  (fp_text value "POT_IN_1" (at 6.05 5.15) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 424b07d8-1c7d-46d4-aef8-a503abfcaec3)
  )
  (fp_line (start 0.94 0.825) (end 0.94 2.46) (layer "F.SilkS") (width 0.12) (tstamp 1acab943-1129-4e94-bdf5-66775e188ae1))
  (fp_line (start 0.94 -4.175) (end 0.94 -3.325) (layer "F.SilkS") (width 0.12) (tstamp 29698152-320d-4905-918d-a6b66dddba1a))
  (fp_line (start 0.94 -1.675) (end 0.94 -0.825) (layer "F.SilkS") (width 0.12) (tstamp 337e82dd-e205-48b7-acc1-60325cd3b3df))
  (fp_line (start 13.06 -7.461) (end 13.06 2.46) (layer "F.SilkS") (width 0.12) (tstamp 33c02b0f-7b68-4b34-926c-bf7248d682bf))
  (fp_line (start 0.94 -7.461) (end 4.806 -7.461) (layer "F.SilkS") (width 0.12) (tstamp abaccd29-54d2-45bc-986d-ac76c43b523d))
  (fp_line (start 9.195 -7.461) (end 13.06 -7.461) (layer "F.SilkS") (width 0.12) (tstamp b7073c8b-de70-491f-b384-57222855e846))
  (fp_line (start 0.94 2.46) (end 4.806 2.46) (layer "F.SilkS") (width 0.12) (tstamp cb9e19ec-3462-4e59-af4b-605f71868ce3))
  (fp_line (start 0.94 -7.461) (end 0.94 -5.825) (layer "F.SilkS") (width 0.12) (tstamp da5195d0-145f-4b10-9e8b-bf0d3c6b7500))
  (fp_line (start 9.195 2.46) (end 13.06 2.46) (layer "F.SilkS") (width 0.12) (tstamp f16a886d-928f-46af-9e74-5440017d03b0))
  (fp_arc (start 8.671982 -5.262432) (mid 10.500762 -2.500553) (end 8.673 0.262) (layer "F.SilkS") (width 0.12) (tstamp 321ff93e-45fb-4309-8d5c-3cd0c4ea7ddf))
  (fp_arc (start 5.571705 -0.202247) (mid 4.500335 -2.500192) (end 5.572 -4.798) (layer "F.SilkS") (width 0.12) (tstamp 49adb4b0-19ee-45d5-bfb3-bd6e41a255c5))
  (fp_line (start -1.15 4.15) (end 13.25 4.15) (layer "F.CrtYd") (width 0.05) (tstamp 24fe8ba7-7c86-4224-b8dc-5b378927f5fd))
  (fp_line (start 13.25 4.15) (end 13.25 -9.15) (layer "F.CrtYd") (width 0.05) (tstamp 2af5db0e-84f5-435f-9347-198f3d542701))
  (fp_line (start 13.25 -9.15) (end -1.15 -9.15) (layer "F.CrtYd") (width 0.05) (tstamp c2d4da4f-5707-46ae-8b92-af0f92280ed9))
  (fp_line (start -1.15 -9.15) (end -1.15 4.15) (layer "F.CrtYd") (width 0.05) (tstamp d94b8452-4fc8-47e0-b003-d4c144d5e4c5))
  (fp_line (start 13 2.4) (end 13 -7.4) (layer "F.Fab") (width 0.1) (tstamp 2e885732-c4e6-4b25-9092-f8558ab691f7))
  (fp_line (start 1 2.4) (end 13 2.4) (layer "F.Fab") (width 0.1) (tstamp a403403c-e258-4451-a913-26c34a6047b3))
  (fp_line (start 1 -7.4) (end 1 2.4) (layer "F.Fab") (width 0.1) (tstamp ca907a4b-73ab-412a-9c15-1b90fc7c62ea))
  (fp_line (start 13 -7.4) (end 1 -7.4) (layer "F.Fab") (width 0.1) (tstamp cef11178-e301-4ae8-9231-fe712e031178))
  (fp_circle (center 7.5 -2.5) (end 10.75 -2.5) (layer "F.Fab") (width 0.1) (fill none) (tstamp 9c7e9aaf-5d42-4806-8a79-5702e8bf7be9))
  (fp_circle (center 7.5 -2.5) (end 10.5 -2.5) (layer "F.Fab") (width 0.1) (fill none) (tstamp bcc50589-cbe3-4f7c-8e03-e30cc863e565))
  (pad "" np_thru_hole circle (at 7 -6.9) (size 4 4) (drill 2.2) (layers F&B.Cu *.Mask) (tstamp 3f5a3131-a054-4ca7-a30a-adb3b990b05c))
  (pad "" np_thru_hole circle (at 7 1.9) (size 4 4) (drill 2.2) (layers F&B.Cu *.Mask) (tstamp 692c3df1-2592-4394-bfa2-e6db8b347e8b))
  (pad "1" thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask) (tstamp 3c546746-a69d-4991-805d-a030786ebba8))
  (pad "2" thru_hole circle (at 0 -2.5) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask) (tstamp 8e744a9a-b2d1-44f5-851e-baadc63594bd))
  (pad "3" thru_hole circle (at 0 -5) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask) (tstamp 4c03e767-4f50-4f7e-b433-0973a8908041))
  (model "Potentiometers.3dshapes/Potentiometer_Alps_RK09K_Horizontal.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 0.393701 0.393701 0.393701))
    (rotate (xyz 0 0 0))
  )
  (model "/home/timcaldwell/projects/kicad-3dmodels/9mm-potentiometer-tall-trimmer-1.snapshot.4/R-0904N-L-25KCv2.step"
    (offset (xyz 7 2.5 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 -90))
  )
)
